===============================================================================
                                  USB-i485
                      Novus Produtos Eletronicos Ltda
                          www.novusautomation.com
===============================================================================

THIS CD CONTAINS THE MANUAL AND DRIVER PACKAGE V 1.7:
- USB-i485 USB drivers (folder "Drivers").
- Installation and Operation instructions (folder "Docs\English").

INSTALLATION

The following installation steps may be slightly different depending on your PC 
configuration and Windows version. Follow the Wizard instructions and use the 
following steps and figures to select the correct installation options.

WINDOWS 98 / ME / 2000

1.	Insert the USB-i485 CD in the CD-ROM drive.
2.	Connect the module to a PC USB port. Windows® will detect the new hardware 
and after a few seconds the Add New Hardware Wizard will start. Select “Next”.
3.	Select “Search for the best driver for your device (Recommended)” and 
select “Next”.
4.	Select option “CD-ROM drive”. If the installation files are not in a CD, 
select option “Specify a location” and type the path for the required files. 
Select “Next”.
5.	Select “Next” when Windows® is ready to install the driver.
6.	The USB-i485 driver files will be copied to your computer and, when 
concluded, a window will show up informing that the wizard has finished 
installing the software. Select “Finish”.
7.	It is possible that the previous steps repeat a second time for the 
completion of installation.

In future connection of USB-i485 modules, it is possible that Windows® prompt 
again for the USB driver installation. In this case, the same wizard will be 
presented. Follow the above steps, but check no options in step 4, since the 
driver files are already in your computer.

WINDOWS XP

1.	Insert the USB-i485 CD in the CD-ROM drive.
2.	Connect the module to a PC USB port. Windows® will detect the new hardware 
and after a few seconds the new hardware wizard will start.
3.	The Found New Hardware Wizard will show-up and ask if you want to connect 
to Windows Update to get the driver. Select the “No, not this time” and 
select “Next”.
4.	Select “Install from a list or specific location (advanced)” and 
select “Next”.
5.	Select “Search for the best driver in these locations” and check option 
“Search removable media”. Select “Next”. If the installation files are not in a CD, 
select option “Include this location in the search” and type the path for 
the required files.
6.	If a warning message regarding Windows® XP compatibility appears, 
select “Continue Anyway”.
7.	The USB-i485 driver files will be copied to your computer and, when concluded, 
a window will show up informing that the wizard has finished installing the software. 
Select “Finish”.
8.	It is possible that the previous steps repeat a second time for the 
completion of installation.


In future connection of USB-i485 modules, it is possible that Windows® prompt again 
for the USB driver installation. In this case, the same wizard will be presented. 
Follow the above steps, but select option “Install the software automatically (recommended)”, 
since the driver files are already installed.
